

**OIML TC7 – Measuring Instruments for Length**

**R35-1 Proposed amendment and vote – November 2013**

**Proposal**

Section II, Metrological Requirements, 4.4.1 Temperature, is amended to read:

*The temperature limits shall be the reference temperature +/-8°C or the temperature indicated on the measure +/-8°C.*

*The temperature limits of +/-8°C shall be disregarded if there is a thermal expansion coefficient marked on the measure or if the measure carries temperature correction information. In this way for each measurement taken the change of length at the working temperature can be calculated and confirmed.*


Clause 6.2 should be amended to eliminate ‘.....*plus all other errors*.....’ for the above reasons and because it would contradict 4.4.1.

**Proposal 2**

To leave the requirements unchanged from the 2007 edition.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Please consider the two proposals and return your votes and any other comments to the TC7 Secretariat at [christine.munteanu@nmo.gov.uk](mailto:christine.munteanu@nmo.gov.uk) by the **31st December 2013**.



**OIML TC7 – Measuring Instruments for Length**

**R35-1 Proposed amendment and vote – November 2013**

|  |  |  |  |
| --- | --- | --- | --- |
| **Proposal** | **For** | **Against** | **Abstention** |
| **Proposal 1** |  |  |  |
| **Proposal 2** |  |  |  |

Member State:

Representative’s name:

Signature:

Date:

|  |
| --- |
| Other comments: |
|  |

Return to [christine.munteanu@nmo.gov.uk](mailto:christine.munteanu@nmo.gov.uk)